***Warranty***

The warranty covers the equipment and components incorporated by Mech-Chem Associates, Inc for the «SYSTEM» being constructed for «COMPANY», in «TOWN», «STATE». The components are warranted against workmanship defects for a period of one (1) year from the date of delivery to «COMPANY».  Vendor components and equipment carry their own manufacturers’ pass through warranty.

Mech-Chem Associates, Inc. does not accept responsibility in connection with equipment altered by others without our written consent or if the System is used outside the original operational specifications.

Mech-Chem is not responsible for labor, use of utilities, removal / storage of chemistry, shipping or other costs incurred by the facility due to defects or faulty equipment. Mech-Chem is also not liable for any loss of production or down time. Plant Personnel must be willing to perform or assist Mech-Chem with any tasks required while dealing with and rectifying any warranty issues. This includes, but is not limited to, labor, removal of and installation of new equipment or materials, as well as decontaminating packaging and shipping of materials and components.

Manufacturer warranties require materials to be returned (free of chemistry and neutralized) to the factory for their review. This requires the removed component to be replaced with spare parts that «COMPANY» is to maintain. Mech-Chem will work on the behalf of «COMPANY» to verify all correct steps are taken to ensure replacement from the manufacturer. The manufacturer has final say over any replacement costs if they deem the failure was not due to a manufacturers’ defect or the part is out of warranty.

«COMPANY» is to maintain an inventory of spare parts, to aid with quick repairs and minimize prolonged periods of equipment down time.

«COMPANY» is to maintain the system in good working condition and perform Preventative Maintenance on a periodic bases, or as spelled out by equipment manufacturer specifications.

***Clause on Acid Recovery Systems***

Due to the proprietary nature of the chemistry, and varying production rates, the frequency at which the stacks will have to be serviced will vary. Proper maintenance of the filtration system and frequent inspection of the Water and Acid tanks for signs of particulate or sediment is critical to the functionality of the system. Any pre or post precipitation due to fluctuation of chemistry or external conditions are not the responsibility of Mech-Chem.

***SPARE PARTS***

«COMPANY» must maintain spare parts inventory which includes items that could shut down production, materials that have multiple application, and long lead time components.

The spare parts will be used for several applications:

1. Spare Part inventory will be used to replace the material or equipment that is no longer functioning properly. Once «COMPANY» has replaced the product it is to be mailed to Mech-Chem, free of chemistry or residue, for evaluation. Criteria spelled out in the Warranty section apply to replacement of components.
2. Spare Part inventory will be used during Preventative Maintenance of System to replace components that are considered wear items. Wear items have to be rebuilt or replaced in a specified time period or on a periodic time basis (some items are quarterly, semiannually or annually).

***PREVENTATIVE MAINTENACE***

«COMPANY» is to maintain the system in good working condition and perform Preventative Maintenance on a periodic bases, or as spelled out by equipment manufacture specifications.

It is recommended for the Acid Recovery Systems that the customer contract with Mech-Chem to perform regular preventative maintenance and site inspections.